DLC pro LabVIEW demonstration 2.0.1
-----------------------------------

Requires LabVIEW 2016 or higher.

The software provides LabVIEW VIs for the operation of the 
DLC pro. Moreover, example program serve for a quick start 
and demonstrate how these VIs are put into action.

The folder “example” provides two examples.

The folder “DLCpro” provides the DLCpro-class and the 
related VIs used by the examples.

The folder “DeCOF” provides the lower level VIs, i.e. the 
DLCpro-class uses the VIs in this folder.


The three examples provided are:
- "DLC_DLpro_simple_example.vi":
  Simple example, addressing a DLC pro controlling a DL pro.

- "DLC_DL_example.vi":
  Also for a addressing a DLC pro controlling a DL pro with 
  more functionality demonstrated.

- "DLC SHG_Example.vi":
  An example for connecting to a DLC pro controlling a 
  NLO system, including access to the AutoAlign procedure.

For an overview of the functionality accessible through the 
DLC pro interface, please see the “Command Reference”, 
which is provided in the “Documentation” folder of any 
DLC pro software release. If you need access to functionality 
that is not provided with the VIs of the “DLCpro” class, you 
can simply use of the DeCOF “parameter_get”, “parameter_set” 
and “command_execute” VIs to send remote commands to the 
DLC pro (see "Command Reference") after you have established 
the connection to the DLC pro.

Happy programming and best regards,
your DLC pro team


TOPTICA Photonics AG
10.08.2020
